YY-Y0152

Solar Panel: 6V 500ma 3W

Battery:3.7v 4400mah Li-ion Battery

Light Source: 38pcs LED SMD2835

Light Power: 3W

Charging time: 8 Hours

Working time: >12 Hours

Material: ABS,PC,Aluminum

IP Rate: IP65

Sensor distance: 6-12M

Output Lumen:600lm

Product Size：260\*160\*110MM

**Package Included:**
1 x LED Solar Light
2 x Expansion Pillar-hinge
2 x Screw
1 x Key Pin
1 x User Manual

**Product Application Area:**
\* Corridor
\* Mailbox
\* Garden
\* Fence
\* Park
\* Patio
\* Deck
\* Yard
\* Home
\* Driveway
\* Stairs
\* Outside Wall

When people coming near the light will turn on for 30 seconds,when people leave,the lamp will switch off automatically .

<http://www.amazon.com/OTTFF-Solar-Motion-Sensor-Nightlight/dp/B00MUT52HK/>